1. **Purpose of this Equipment:** To clean eyes, face, hands and body with a controlled spray of potable water in the event of an accidental contamination.
2. **Federal Supply Class:** 6515
3. **General Operating Specifications:**
   1. **Dimensions:** 
      1. The length of the drench hose is to be a minimum of eight feet.
   2. **Salient Characteristics that shall be provided:**
      1. Dual stream heads with covers.
      2. Stay open (no use of hands) valve assembly.
      3. Hose connection reinforced PVC hose, 300 PSI maximum working pressure.
      4. Supply .375 (3/8) inch iron pipe size (IPS) male thread.
      5. Wall Mount Hood for the spray head.
      6. Sign ANSI-compliant identification sign.

# Industry Standards / Requirement(s):

* + 1. **Industry Standards:**American National Standards Institute**(**ANSI Standard Z358.1)
    2. Warranty period shall be for (1) year from date of delivery/installation against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to make utility connections, mount, assemble and use.
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements:** N / A

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

