# Purpose of this Equipment: To accommodate 12 inch platters or pans for moving product.

1. **Federal Supply Class:** 7320
2. **General Operating Specifications:**
   1. **Dimensions:** 
      1. 26 inches long / wide, 18 inches deep, 70 inches high. Dimensional sizes of +/- 3 inches are acceptable. The runners must be able to hold 12 inch wide platters or pans.
   2. **Salient Characteristics that shall be provided:**
      1. All Stainless steel construction.
      2. 1 ½ inch angle runners with six inch spacing.
      3. Accommodate 10 platters or pans.
      4. All four wheels to be swivel casters.
      5. 5 inches in diameter, polyurethane wheels.

# Industry Standards / Requirement(s):

* + 1. Industry Standards: National Sanitation Foundation (NSF) certification, or approved equivalent. Conformité Européene (CE) is not acceptable for a standard.
    2. Warranty period shall be for (1) year from date of delivery against defective material and workmanship and shall include parts, service and labor.
  1. **Information Technology requirements:** N / A

# Color Requirement(s): N / A

1. **Electrical Requirements:** N / A

# Standard Contractor Requirements:

* 1. Must be shipped ready to use.
  2. **Information to be provided by the Contractor to the commissary at the time of delivery:**
     1. Point of Contact for Service
     2. Installation and Operating Instructions
     3. Parts List
  3. **Maintenance Sustainability Requirements:** Continued parts support is required for the projected life cycle of the equipment plus 5 years.

# Special Coordinating / Safety Instructions: N / A

**STORE ORDER REQUEST**

**STORE NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DODAAC: ­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**QUANTITY: \_\_\_\_\_\_\_**

****